IFC building model
Schema: "IFC2X3"
Time stamp: "2021-10-26T09:23:52"
Preprocessor: "Processor version 5.1.0.0"
Originating system: "Xbim.IO.MemoryModel"
Application: "VK-torustikud" by Organization (no name given)

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "VK-torustikud" by Organization (no name given) | change ADDED | created 0 (1970-01-01T00:00:00Z) | last modified 1635240233 (2021-10-26T09:23:53Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "1Cj6oYHHv8VfpgmpDVy5nq"
  IFCBUILDING "Building"

Property sets
  Toru | properties | on 1 object (1 IFCFLOWSEGMENT)
    ALUS = "" (IFCTEXT)
    DIAMETER = 110. (IFCNUMERICMEASURE)
    FROM = "KLV-141" (IFCTEXT)
    FROM_X = 543306.235 (IFCNUMERICMEASURE)
    FROM_Y = 6589701.707 (IFCNUMERICMEASURE)
    FROM_Z = 1.81 (IFCNUMERICMEASURE)
    GRADIENT = 0.093 (IFCNUMERICMEASURE)
    KONSTR = "" (IFCTEXT)
    LENGTH = 5.711 (IFCNUMERICMEASURE)
    MATERIAL = "De110" (IFCTEXT)
    NETWORK = "sadekanal" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    TO = "SK-137" (IFCTEXT)
    TO_X = 543310.774 (IFCNUMERICMEASURE)
    TO_Y = 6589698.81 (IFCNUMERICMEASURE)
    TO_Z = 1.28 (IFCNUMERICMEASURE)
    TYPE = "kinnistutoru" (IFCTEXT)
  Toru | properties | on 1 object (1 IFCFLOWSEGMENT)
    ALUS = "" (IFCTEXT)
    DIAMETER = 110. (IFCNUMERICMEASURE)
    FROM = "KLV-142" (IFCTEXT)
    FROM_X = 543311.527 (IFCNUMERICMEASURE)
    FROM_Y = 6589703.685 (IFCNUMERICMEASURE)
    FROM_Z = 1.81 (IFCNUMERICMEASURE)
    GRADIENT = 0.013 (IFCNUMERICMEASURE)
    KONSTR = "" (IFCTEXT)
    LENGTH = 2.965 (IFCNUMERICMEASURE)
    MATERIAL = "De110" (IFCTEXT)
    NETWORK = "sadekanal" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    TO = "SK-156" (IFCTEXT)
    TO_X = 543314.299 (IFCNUMERICMEASURE)
    TO_Y = 6589704.737 (IFCNUMERICMEASURE)
    TO_Z = 1.77 (IFCNUMERICMEASURE)
    TYPE = "kinnistutoru" (IFCTEXT)
  Toru | properties | on 1 object (1 IFCFLOWSEGMENT)
    ALUS = "" (IFCTEXT)
    DIAMETER = 110. (IFCNUMERICMEASURE)
    FROM = "KLV-143" (IFCTEXT)
    FROM_X = 543322.103 (IFCNUMERICMEASURE)
    FROM_Y = 6589707.664 (IFCNUMERICMEASURE)
    FROM_Z = 1.81 (IFCNUMERICMEASURE)
    GRADIENT = 0.013 (IFCNUMERICMEASURE)
    KONSTR = "" (IFCTEXT)
    LENGTH = 2.965 (IFCNUMERICMEASURE)
    MATERIAL = "De110" (IFCTEXT)
    NETWORK = "sadekanal" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    TO = "SK-157" (IFCTEXT)
    TO_X = 543324.879 (IFCNUMERICMEASURE)
    TO_Y = 6589708.705 (IFCNUMERICMEASURE)
    TO_Z = 1.77 (IFCNUMERICMEASURE)
    TYPE = "kinnistutoru" (IFCTEXT)
  Toru | properties | on 1 object (1 IFCFLOWSEGMENT)
    ALUS = "" (IFCTEXT)
    DIAMETER = 110. (IFCNUMERICMEASURE)
    FROM = "KLV-146" (IFCTEXT)
    FROM_X = 543332.68 (IFCNUMERICMEASURE)
    FROM_Y = 6589711.643 (IFCNUMERICMEASURE)
    FROM_Z = 1.81 (IFCNUMERICMEASURE)
    GRADIENT = 0.013 (IFCNUMERICMEASURE)
    KONSTR = "" (IFCTEXT)
    LENGTH = 2.965 (IFCNUMERICMEASURE)
    MATERIAL = "De110" (IFCTEXT)
    NETWORK = "sadekanal" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    TO = "SK-165" (IFCTEXT)
    TO_X = 543335.455 (IFCNUMERICMEASURE)
    TO_Y = 6589712.686 (IFCNUMERICMEASURE)
    TO_Z = 1.77 (IFCNUMERICMEASURE)
    TYPE = "kinnistutoru" (IFCTEXT)
  Toru | properties | on 1 object (1 IFCFLOWSEGMENT)
    ALUS = "" (IFCTEXT)
    DIAMETER = 110. (IFCNUMERICMEASURE)
    FROM = "SK-165" (IFCTEXT)
    FROM_X = 543335.455 (IFCNUMERICMEASURE)
    FROM_Y = 6589712.686 (IFCNUMERICMEASURE)
    FROM_Z = 1.23 (IFCNUMERICMEASURE)
    GRADIENT = 0.009 (IFCNUMERICMEASURE)
    KONSTR = "" (IFCTEXT)
    LENGTH = 4.3 (IFCNUMERICMEASURE)
    MATERIAL = "De110" (IFCTEXT)
    NETWORK = "sadekanal" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    TO = "SK-138" (IFCTEXT)
    TO_X = 543336.967 (IFCNUMERICMEASURE)
    TO_Y = 6589708.661 (IFCNUMERICMEASURE)
    TO_Z = 1.19 (IFCNUMERICMEASURE)
    TYPE = "kinnistutoru" (IFCTEXT)
  Toru | properties | on 1 object (1 IFCFLOWSEGMENT)
    ALUS = "" (IFCTEXT)
    DIAMETER = 110. (IFCNUMERICMEASURE)
    FROM = "KLV-163" (IFCTEXT)
    FROM_X = 543336.183 (IFCNUMERICMEASURE)
    FROM_Y = 6589712.953 (IFCNUMERICMEASURE)
    FROM_Z = 1.66 (IFCNUMERICMEASURE)
    GRADIENT = 0.013 (IFCNUMERICMEASURE)
    KONSTR = "" (IFCTEXT)
    LENGTH = 0.775 (IFCNUMERICMEASURE)
    MATERIAL = "De110" (IFCTEXT)
    NETWORK = "sadekanal" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    TO = "SK-165" (IFCTEXT)
    TO_X = 543335.455 (IFCNUMERICMEASURE)
    TO_Y = 6589712.686 (IFCNUMERICMEASURE)
    TO_Z = 1.65 (IFCNUMERICMEASURE)
    TYPE = "kinnistutoru" (IFCTEXT)
  Toru | properties | on 1 object (1 IFCFLOWSEGMENT)
    ALUS = "" (IFCTEXT)
    DIAMETER = 160. (IFCNUMERICMEASURE)
    FROM = "SK-157" (IFCTEXT)
    FROM_X = 543324.879 (IFCNUMERICMEASURE)
    FROM_Y = 6589708.705 (IFCNUMERICMEASURE)
    FROM_Z = 1.23 (IFCNUMERICMEASURE)
    GRADIENT = 0.009 (IFCNUMERICMEASURE)
    KONSTR = "" (IFCTEXT)
    LENGTH = 4.292 (IFCNUMERICMEASURE)
    MATERIAL = "De160" (IFCTEXT)
    NETWORK = "sadekanal" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    TO = "SK-148" (IFCTEXT)
    TO_X = 543326.389 (IFCNUMERICMEASURE)
    TO_Y = 6589704.687 (IFCNUMERICMEASURE)
    TO_Z = 1.19 (IFCNUMERICMEASURE)
    TYPE = "kinnistutoru" (IFCTEXT)
  Toru | properties | on 1 object (1 IFCFLOWSEGMENT)
    ALUS = "" (IFCTEXT)
    DIAMETER = 110. (IFCNUMERICMEASURE)
    FROM = "KLV-148" (IFCTEXT)
    FROM_X = 543325.6 (IFCNUMERICMEASURE)
    FROM_Y = 6589708.992 (IFCNUMERICMEASURE)
    FROM_Z = 1.81 (IFCNUMERICMEASURE)
    GRADIENT = 0.013 (IFCNUMERICMEASURE)
    KONSTR = "" (IFCTEXT)
    LENGTH = 0.776 (IFCNUMERICMEASURE)
    MATERIAL = "De110" (IFCTEXT)
    NETWORK = "sadekanal" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    TO = "SK-157" (IFCTEXT)
    TO_X = 543324.879 (IFCNUMERICMEASURE)
    TO_Y = 6589708.705 (IFCNUMERICMEASURE)
    TO_Z = 1.8 (IFCNUMERICMEASURE)
    TYPE = "kinnistutoru" (IFCTEXT)
  Toru: 35 more contents on 35 objects not shown
  Kaevud | properties | on 2 objects (2 IFCFLOWFITTING)
    ALT = "" (IFCTEXT)
    BOTTOM_Z = 1.23 (IFCNUMERICMEASURE)
    COVER_MAT (no value)
    COVER_TYPE = "kontrollkaev" (IFCTEXT)
    DEPTH = 1.2400000000000002 (IFCNUMERICMEASURE)
    DIAMETER = 400. (IFCNUMERICMEASURE)
    GROUND_Z = 2.47 (IFCNUMERICMEASURE)
    KOMM = "" (IFCTEXT)
    LABEL = "SK-165" (IFCTEXT)
    MATERIAL = "PE400/315" (IFCTEXT)
    NETWORK = "drenaaz" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    X = 543335.455 (IFCNUMERICMEASURE)
    Y = 6589712.686 (IFCNUMERICMEASURE)
  Kaevud | properties | on 2 objects (2 IFCFLOWFITTING)
    ALT = "" (IFCTEXT)
    BOTTOM_Z = 1.23 (IFCNUMERICMEASURE)
    COVER_MAT (no value)
    COVER_TYPE = "kontrollkaev" (IFCTEXT)
    DEPTH = 1.2999999999999998 (IFCNUMERICMEASURE)
    DIAMETER = 400. (IFCNUMERICMEASURE)
    GROUND_Z = 2.53 (IFCNUMERICMEASURE)
    KOMM = "" (IFCTEXT)
    LABEL = "SK-157" (IFCTEXT)
    MATERIAL = "PE400/315" (IFCTEXT)
    NETWORK = "drenaaz" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    X = 543324.879 (IFCNUMERICMEASURE)
    Y = 6589708.705 (IFCNUMERICMEASURE)
  Kaevud | properties | on 2 objects (2 IFCFLOWFITTING)
    ALT = "" (IFCTEXT)
    BOTTOM_Z = 1.23 (IFCNUMERICMEASURE)
    COVER_MAT (no value)
    COVER_TYPE = "kontrollkaev" (IFCTEXT)
    DEPTH = 1.2000000000000002 (IFCNUMERICMEASURE)
    DIAMETER = 400. (IFCNUMERICMEASURE)
    GROUND_Z = 2.43 (IFCNUMERICMEASURE)
    KOMM = "" (IFCTEXT)
    LABEL = "SK-156" (IFCTEXT)
    MATERIAL = "PE400/315" (IFCTEXT)
    NETWORK = "drenaaz" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    X = 543314.299 (IFCNUMERICMEASURE)
    Y = 6589704.737 (IFCNUMERICMEASURE)
  Kaevud | properties | on 2 objects (2 IFCFLOWFITTING)
    ALT = "" (IFCTEXT)
    BOTTOM_Z = 0.98 (IFCNUMERICMEASURE)
    COVER_MAT (no value)
    COVER_TYPE = "kontrollkaev" (IFCTEXT)
    DEPTH = 1.2999999999999998 (IFCNUMERICMEASURE)
    DIAMETER = 400. (IFCNUMERICMEASURE)
    GROUND_Z = 2.28 (IFCNUMERICMEASURE)
    KOMM = "" (IFCTEXT)
    LABEL = "SK-137" (IFCTEXT)
    MATERIAL = "PE400/315" (IFCTEXT)
    NETWORK = "drenaaz" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    X = 543310.774 (IFCNUMERICMEASURE)
    Y = 6589698.81 (IFCNUMERICMEASURE)
  Kaevud | properties | on 2 objects (2 IFCFLOWFITTING)
    ALT = "" (IFCTEXT)
    BOTTOM_Z = 0.948 (IFCNUMERICMEASURE)
    COVER_MAT (no value)
    COVER_TYPE = "kontrollkaev" (IFCTEXT)
    DEPTH = 1.512 (IFCNUMERICMEASURE)
    DIAMETER = 400. (IFCNUMERICMEASURE)
    GROUND_Z = 2.46 (IFCNUMERICMEASURE)
    KOMM = "" (IFCTEXT)
    LABEL = "SK-147" (IFCTEXT)
    MATERIAL = "PE400/315" (IFCTEXT)
    NETWORK = "drenaaz" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    X = 543315.811 (IFCNUMERICMEASURE)
    Y = 6589700.712 (IFCNUMERICMEASURE)
  Kaevud | properties | on 2 objects (2 IFCFLOWFITTING)
    ALT = "" (IFCTEXT)
    BOTTOM_Z = 0.87999999999999989 (IFCNUMERICMEASURE)
    COVER_MAT (no value)
    COVER_TYPE = "kontrollkaev" (IFCTEXT)
    DEPTH = 1.54 (IFCNUMERICMEASURE)
    DIAMETER = 400. (IFCNUMERICMEASURE)
    GROUND_Z = 2.42 (IFCNUMERICMEASURE)
    KOMM = "" (IFCTEXT)
    LABEL = "SK-148" (IFCTEXT)
    MATERIAL = "PE400/315" (IFCTEXT)
    NETWORK = "drenaaz" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    X = 543326.389 (IFCNUMERICMEASURE)
    Y = 6589704.687 (IFCNUMERICMEASURE)
  Kaevud | properties | on 2 objects (2 IFCFLOWFITTING)
    ALT = "" (IFCTEXT)
    BOTTOM_Z = 0.812 (IFCNUMERICMEASURE)
    COVER_MAT (no value)
    COVER_TYPE = "kontrollkaev" (IFCTEXT)
    DEPTH = 1.5679999999999998 (IFCNUMERICMEASURE)
    DIAMETER = 400. (IFCNUMERICMEASURE)
    GROUND_Z = 2.38 (IFCNUMERICMEASURE)
    KOMM = "" (IFCTEXT)
    LABEL = "SK-138" (IFCTEXT)
    MATERIAL = "PE400/315" (IFCTEXT)
    NETWORK = "drenaaz" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    X = 543336.967 (IFCNUMERICMEASURE)
    Y = 6589708.661 (IFCNUMERICMEASURE)
  Kaevud | properties | on 2 objects (2 IFCFLOWFITTING)
    ALT = "" (IFCTEXT)
    BOTTOM_Z = 1.23 (IFCNUMERICMEASURE)
    COVER_MAT (no value)
    COVER_TYPE = "kontrollkaev" (IFCTEXT)
    DEPTH = 1.17 (IFCNUMERICMEASURE)
    DIAMETER = 400. (IFCNUMERICMEASURE)
    GROUND_Z = 2.4 (IFCNUMERICMEASURE)
    KOMM = "" (IFCTEXT)
    LABEL = "SK-163" (IFCTEXT)
    MATERIAL = "PE400/315" (IFCTEXT)
    NETWORK = "drenaaz" (IFCTEXT)
    STATUS = "projekteeritav" (IFCTEXT)
    X = 543356.614 (IFCNUMERICMEASURE)
    Y = 6589720.627 (IFCNUMERICMEASURE)
  Kaevud: 30 more contents on 42 objects not shown