IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "868SILOS_CON_WEST_R22.ifc (Edited by Simplebim 9.1 SR6)"
Time stamp: "2023-02-08T13:24:12"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.6.0.0 - Alternate UI 22.6.0.0"
Application: "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person (no name given) of Organization "Simplebim"
  Person "ricUEH89" of Organization "Pieters Bouwtechniek"
  Owner history of Person (no name given) of Organization "Simplebim" | application "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist" | change ADDED | created 1675859784 (2023-02-08T12:36:24Z)
  Owner history of Person "ricUEH89" of Organization "Pieters Bouwtechniek" | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1675858267 (2023-02-08T12:11:07Z)

Units
  PLANEANGLEUNIT: DEGREE (conversion based)
  AREAUNIT: MILLI SQUARE_METRE
  LENGTHUNIT: MILLI METRE
  MASSUNIT: KILO GRAM
  POWERUNIT: WATT
  PRESSUREUNIT: PASCAL
  FORCEUNIT: KILO NEWTON
  ELECTRICVOLTAGEUNIT: VOLT
  ELECTRICCURRENTUNIT: AMPERE
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  TIMEUNIT: SECOND
  VOLUMEUNIT: MILLI CUBIC_METRE
  LINEARVELOCITYUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  THERMALTRANSMITTANCEUNIT: derived
  SOUNDPRESSUREUNIT: derived

Spatial structure
IFCPROJECT "717138" | long name "Drie Koningen" | phase "Uitvoeringsgereed Ontwerp"
  IFCSITE "Default" | latitude 52° 22′ 22.799999″ | longitude 4° 53′ 41.279999″ | elevation above sea level 0.
    IFCBUILDING "Silo's Drie Koningen Amsterdam" | long name "Silo's Drie Koningen Amsterdam" | postal address: "Amsterdam", "Amsterdam", "Netherlands"
      IFCBUILDINGSTOREY "07 zevende verdieping" | long name "07 bk ruwe vloer laag 2" | object type "Level:PBT_level" | elevation 31510.
        contains 1 element
          1 x IFCSLAB | type IFCSLABTYPE "Floors : Floor : 23_PBT_FL_staalplaatbeton_d=290" | object type "Floor:23_PBT_FL_staalplaatbeton_d=290" | FLOOR | names: "Floors : Floor : 23_PBT_FL_staalplaatbeton_d=290" | material: layers "Floor:23_PBT_FL_staalplaatbeton_d=290" ("00_PBT_MAT_Beton t.p.g." 290.) | property sets: Pset_SlabCommon, Pset_ConcreteElementGeneral, Pset_ProductRequirements, Pset_ReinforcementBarPitchOfSlab, Pset_QuantityTakeOff, ePset_Simplebim

Types
  IFCSLABTYPE "Floors : Floor : 23_PBT_FL_staalplaatbeton_d=290" | FLOOR | 1 occurrence | material: layers "Floor:23_PBT_FL_staalplaatbeton_d=290" ("00_PBT_MAT_Beton t.p.g." 290.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon

Property sets
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Category = "Floors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "07 bk ruwe vloer laag 2" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "07 bk ruwe vloer laag 2" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    FireRating = "60" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Floor:23_PBT_FL_staalplaatbeton_d=290" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCSLAB)
    FireRating = "60" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Floor:23_PBT_FL_staalplaatbeton_d=290" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 type object
    Description = "staalplaat-betonvloer" (IFCTEXT)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCSLAB)
    Reference = "Floor:23_PBT_FL_staalplaatbeton_d=290" (IFCIDENTIFIER)
  ePset_Simplebim | properties | on 1 object (1 IFCSLAB)
    Assembly Level = "Single" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 1 type object
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]