IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "RevitIdentifiers [VersionGUID: 1b09f447-5f92-4aca-914f-a756c175cfa7, NumberOfSaves: 15]"
Description: "ExchangeRequirement [Architecture]"
Description: "CoordinateReference [CoordinateBase: Aktuelle gemeinsam genutzte Koordinaten, ProjectSite: Intern]"
File name: "2018_01"
Time stamp: "2023-04-12T12:10:16+01:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "23.1.10.4 - Exporter 23.2.5.0 - Alternative Benutzeroberfläche 23.2.5.0"
Application: "Autodesk Revit 2023 (DEU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (DEU)"

People and organizations
  Person "m.muellerKN4YQ" of Organization (no name given)
  Owner history of Person "m.muellerKN4YQ" of Organization (no name given) | application "Autodesk Revit 2023 (DEU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (DEU)" | change NOCHANGE | created 1673986166 (2023-01-17T20:09:26Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  CURRENCY: €
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived

Spatial structure
IFCPROJECT "2018_01" | phase "Projekt Status"
  IFCSITE "Default" | latitude 48° 8′ 15.359802″ | longitude 11° 34′ 47.783432″ | elevation above sea level 0.
    contains 16 elements
      1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:STB 200" | object type "Geschossdecke:STB 200" | names: "Geschossdecke:STB 200:2414458" | parts: 1 IFCBUILDINGELEMENTPART | property sets: Qto_SlabBaseQuantities
      1 x IFCFOOTING | type IFCFOOTINGTYPE "STB Träger - rechteckig:Streifenfundament" | object type "STB Träger - rechteckig:Streifenfundament" | STRIP_FOOTING | names: "STB Träger - rechteckig:Streifenfundament:2416361" | material: "Ortbeton - bewehrt Verputzt" | property sets: Qto_FootingBaseQuantities
      2 x IFCBEAM | type IFCBEAMTYPE "Basiswand:Streifenfundament Wand" | object type "Basiswand:Streifenfundament Wand" | names: "Basiswand:Streifenfundament Wand:2416447", "Basiswand:Streifenfundament Wand:2418437" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2416606" | material: "Ortbeton - bewehrt Verputzt" | property sets: Qto_BeamBaseQuantities
      2 x IFCWINDOW | type IFCWINDOWTYPE "FE 1 tlg - DrehKipp:1100 x 1400" | object type "FE 1 tlg - DrehKipp:1100 x 1400" | WINDOW | names: "FE 1 tlg - DrehKipp:1100 x 1400:2416967", "FE 1 tlg - DrehKipp:1100 x 1400:2418438" | material: constituents ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Qto_WindowBaseQuantities
      2 x IFCCOLUMN | type IFCCOLUMNTYPE "IPE Stütze:IPE 300" | object type "IPE Stütze:IPE 300" | COLUMN | names: "IPE Stütze:IPE 300:2417116", "IPE Stütze:IPE 300:2417144" | material: "Metall - Baustahl S235" | property sets: Qto_ColumnBaseQuantities
      2 x IFCWALL | type IFCWALLTYPE "Basiswand:GK 100" | object type "Basiswand:GK 100" | names: "Basiswand:GK 100:2417328", "Basiswand:GK 100:2418441" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Qto_WallBaseQuantities
      3 x IFCWALL | type IFCWALLTYPE "Basiswand:Ziegel+WD hart 200+200" | object type "Basiswand:Ziegel+WD hart 200+200" | names: "Basiswand:Ziegel+WD hart 200+200:2417837", "Basiswand:Ziegel+WD hart 200+200:2417963", "Basiswand:Ziegel+WD hart 200+200:2418442" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Qto_WallBaseQuantities
      2 x IFCCOLUMN | type IFCCOLUMNTYPE "IPE Stütze:IPE 300" | object type "IPE Stütze:IPE 300" | COLUMN | names: "IPE Stütze:IPE 300:2418439", "IPE Stütze:IPE 300:2418440" | material: "Metall - Baustahl S235" | property sets: Qto_ColumnBaseQuantities

Types
  IFCSLABTYPE "Geschossdecke:STB 200" | 1 occurrence
  IFCFOOTINGTYPE "STB Träger - rechteckig:Streifenfundament" | STRIP_FOOTING | 1 occurrence | material: "Ortbeton - bewehrt Verputzt"
  IFCBEAMTYPE "Basiswand:Streifenfundament Wand" | 2 occurrences
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: "Ortbeton - bewehrt Verputzt"
  IFCWINDOWTYPE "FE 1 tlg - DrehKipp:1100 x 1400" | WINDOW | 2 occurrences | material: constituents ("Sichtbeschläge": "Metall - Edelstahl gebürstet", "Element/Flügel": "Kunststoff - grau 70-70-70", "Glas": "Glas - Isolierverglasung klar", "Fensterbank Aussen Blech": "Kunststoff - grau 70-70-70", "Rahmen/Pfosten": "Kunststoff - grau 70-70-70", "Fensterbank Innen": "Holz - generisch 140-100-70") | property sets: FE 1 tlg - DrehKipp:1100 x 1400:2416967
  IFCCOLUMNTYPE "IPE Stütze:IPE 300" | COLUMN | 2 occurrences | material: "Metall - Baustahl S235"
  IFCWALLTYPE "Basiswand:GK 100" | STANDARD | 2 occurrences
  IFCWALLTYPE "Basiswand:Ziegel+WD hart 200+200" | STANDARD | 3 occurrences
  IFCCOLUMNTYPE "IPE Stütze:IPE 300" | COLUMN | 2 occurrences | material: "Metall - Baustahl S235"

Property sets
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetVolume = 13.800000000000004 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 1.7500000000000235 [SQUARE_METRE]
    GrossSurfaceArea = 18.00000000000005 [SQUARE_METRE]
    GrossVolume = 1.7500000000000231 [CUBIC_METRE]
    Height = 0.25000000000000333 [METRE]
    Length = 0.99999999999999967 [METRE]
    NetVolume = 1.7500000000000215 [CUBIC_METRE]
    OuterSurfaceArea = 14.500000000000004 [SQUARE_METRE]
    Width = 7.0000000000000009 [METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 13.020000000000019 [SQUARE_METRE]
    NetSurfaceArea = 30.240000000002432 [SQUARE_METRE]
    NetVolume = 2.603999999999508 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 0.075000000000001885 [SQUARE_METRE]
    GrossSurfaceArea = 11.150000000000786 [SQUARE_METRE]
    GrossVolume = 0.75000000000001898 [CUBIC_METRE]
    Length = 10. [METRE]
    NetSurfaceArea = 11.15000000000011 [SQUARE_METRE]
    NetVolume = 0.75000000000001488 [CUBIC_METRE]
    OuterSurfaceArea = 11.000000000000782 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 13.020000000000014 [SQUARE_METRE]
    NetSurfaceArea = 30.240000000002425 [SQUARE_METRE]
    NetVolume = 2.603999999999508 [CUBIC_METRE]
  Qto_WindowBaseQuantities | quantities | on 2 objects (2 IFCWINDOW)
    Area = 1.54 [SQUARE_METRE]
  Qto_ColumnBaseQuantities | quantities | on 4 objects (4 IFCCOLUMN)
    CrossSectionArea = 0.0053826958672884952 [SQUARE_METRE]
    GrossVolume = 0.015071548428407787 [CUBIC_METRE]
    Length = 2.8000000000000003 [METRE]
    NetVolume = 0.014526568000000005 [CUBIC_METRE]
    OuterSurfaceArea = 3.2481337829015442 [SQUARE_METRE]
  Qto_WallBaseQuantities | quantities | on 3 objects (3 IFCWALL)
    NetVolume = 2.2400000000000007 [CUBIC_METRE]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    NetVolume = 1.0130770000000007 [CUBIC_METRE]
  FE 1 tlg - DrehKipp:1100 x 1400:2416967 | predefined | on 1 type object