IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "Option [BaseQuantities:On]"
Description: "Option [GridExport:On]"
Description: "Option [Assemblies:On]"
Description: "Option [Bolts:On]"
Description: "Option [Rebars:On]"
Description: "Option [PourObjects:Off]"
Description: "Option [Welds:On]"
Description: "Option [SurfaceTreatments:On]"
Description: "Option [LocationBy:0]"
Description: "Option [ViewColors:Off]"
Description: "Option [SectionedSpine:Off]"
Description: "Option [PropertySets:On]"
Description: "Option [Export all:Off]"
File name: "STRUTTURA_ESEMPIO.ifc"
Time stamp: "2023-06-26T15:34:12"
Author: "HARPA\monte"
Organization: "Structural Designer"
Preprocessor: "IFC Database Version: Work"
Originating system: "Tekla Structures 2019 Service Pack 13, IFC Export Version: 4.0.0.0 Oct 18 2021"
Application: "Tekla Structures" version "2019 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

People and organizations
  Person "Undefined" id "HARPA\monte" of Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "HARPA\monte" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2019 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1687786450 (2023-06-26T13:34:10Z)
  Owner history of Person "Undefined" id "HARPA\monte" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2019 Service Pack 13" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1687791600 (2023-06-26T15:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Progetto"
  IFCSITE "Cantiere"
    IFCBUILDING "Undefined"
      IFCBUILDINGSTOREY "Undefined" | elevation 0.
    IFCBUILDING "Edificio"
      contains 3 elements
        3 x IFCGRID | names: "+7200", "+3600", "+0"
      IFCBUILDINGSTOREY "Livello 1" | elevation 0.
        contains 373 elements
          360 x IFCFASTENER | names: "Weld" | property sets: Tekla Weld Common, Tekla Weld Above Line, Tekla Weld Below Line
          13 x IFCELEMENTASSEMBLY | RIGID_FRAME | names: "COLUMN", "BEAM" | parts: 132 IFCDISCRETEACCESSORY, 28 IFCMECHANICALFASTENER, 7 IFCBEAM, 6 IFCCOLUMN | property sets: BaseQuantities, Tekla Assembly
      IFCBUILDINGSTOREY "Livello 2" | elevation 3600.
        contains 127 elements
          102 x IFCFASTENER | names: "Weld" | property sets: Tekla Weld Common, Tekla Weld Above Line, Tekla Weld Below Line
          25 x IFCELEMENTASSEMBLY | RIGID_FRAME | names: "BEAM", "COLUMN", "PIATTO" | parts: 50 IFCDISCRETEACCESSORY, 42 IFCMECHANICALFASTENER, 7 IFCBEAM, 2 IFCCOLUMN | property sets: BaseQuantities, Tekla Assembly

Property sets
  Tekla Assembly | properties | on 4 objects (4 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "A/2" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+4.872" (IFCLABEL)
    Assembly/Cast unit position code = "2/C" (IFCLABEL)
    Assembly/Cast unit top elevation = "+5.332" (IFCLABEL)
    Assembly/Cast unit weight = 2.5 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 4 objects (4 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "A/2" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+4.872" (IFCLABEL)
    Assembly/Cast unit position code = "1/C" (IFCLABEL)
    Assembly/Cast unit top elevation = "+5.332" (IFCLABEL)
    Assembly/Cast unit weight = 2.5 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "A/3" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+4.947" (IFCLABEL)
    Assembly/Cast unit position code = "2/C" (IFCLABEL)
    Assembly/Cast unit top elevation = "+5.257" (IFCLABEL)
    Assembly/Cast unit weight = 2.3 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "A/1" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+4.872" (IFCLABEL)
    Assembly/Cast unit position code = "2/C" (IFCLABEL)
    Assembly/Cast unit top elevation = "+5.332" (IFCLABEL)
    Assembly/Cast unit weight = 7.4 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "A/3" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+4.947" (IFCLABEL)
    Assembly/Cast unit position code = "1/C" (IFCLABEL)
    Assembly/Cast unit top elevation = "+5.257" (IFCLABEL)
    Assembly/Cast unit weight = 2.3 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "A/1" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+4.872" (IFCLABEL)
    Assembly/Cast unit position code = "1/C" (IFCLABEL)
    Assembly/Cast unit top elevation = "+5.332" (IFCLABEL)
    Assembly/Cast unit weight = 7.4 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "B/2" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+6.880" (IFCLABEL)
    Assembly/Cast unit position code = "1-2/C" (IFCLABEL)
    Assembly/Cast unit top elevation = "+7.230" (IFCLABEL)
    Assembly/Cast unit weight = 285.7 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "C/7" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+5.102" (IFCLABEL)
    Assembly/Cast unit position code = "2/C" (IFCLABEL)
    Assembly/Cast unit top elevation = "+7.230" (IFCLABEL)
    Assembly/Cast unit weight = 309.7 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Cast unit type (no value)
    Control number (no value)
  Tekla Assembly: 20 more contents on 20 objects not shown
  BaseQuantities | quantities | on 32 objects (32 IFCDISCRETEACCESSORY)
    CrossSectionArea = 0.0004 [SQUARE_METRE]
    GrossArea = 0.04928 [SQUARE_METRE]
    GrossVolume = 0.00097102 [CUBIC_METRE]
    NetArea = 0.116149350647363 [SQUARE_METRE]
    NetVolume = 0.00097102 [CUBIC_METRE]
  BaseQuantities | quantities | on 24 objects (24 IFCDISCRETEACCESSORY)
    CrossSectionArea = 0.000196 [SQUARE_METRE]
    GrossArea = 0.086064 [SQUARE_METRE]
    GrossVolume = 0.001099896 [CUBIC_METRE]
    NetArea = 0.172044802131761 [SQUARE_METRE]
    NetVolume = 0.001099896 [CUBIC_METRE]
  BaseQuantities | quantities | on 24 objects (24 IFCDISCRETEACCESSORY)
    CrossSectionArea = 0.000196 [SQUARE_METRE]
    GrossArea = 0.077 [SQUARE_METRE]
    GrossVolume = 0.001078 [CUBIC_METRE]
    NetArea = 0.16996 [SQUARE_METRE]
    NetVolume = 0.001078 [CUBIC_METRE]
  BaseQuantities | quantities | on 16 objects (16 IFCDISCRETEACCESSORY)
    CrossSectionArea = 0.0001 [SQUARE_METRE]
    GrossArea = 0.0199999999897789 [SQUARE_METRE]
    GrossVolume = 0.000174999999910565 [CUBIC_METRE]
    NetArea = 0.0404142135431026 [SQUARE_METRE]
    NetVolume = 0.000174999999910565 [CUBIC_METRE]
  BaseQuantities | quantities | on 14 objects (14 IFCDISCRETEACCESSORY)
    CrossSectionArea = 0.0001 [SQUARE_METRE]
    GrossArea = 0.0199999999897811 [SQUARE_METRE]
    GrossVolume = 0.000174999999910596 [CUBIC_METRE]
    NetArea = 0.0404142135431091 [SQUARE_METRE]
    NetVolume = 0.000174999999910596 [CUBIC_METRE]
  BaseQuantities | quantities | on 12 objects (12 IFCELEMENTASSEMBLY)
    Width = 10. [MILLI METRE]
  BaseQuantities | quantities | on 12 objects (12 IFCDISCRETEACCESSORY)
    CrossSectionArea = 0.000196 [SQUARE_METRE]
    GrossArea = 0.064059 [SQUARE_METRE]
    GrossVolume = 0.000871626 [CUBIC_METRE]
    NetArea = 0.137715878784787 [SQUARE_METRE]
    NetVolume = 0.000871626 [CUBIC_METRE]
  BaseQuantities | quantities | on 12 objects (12 IFCDISCRETEACCESSORY)
    CrossSectionArea = 0.006 [SQUARE_METRE]
    GrossArea = 0.406748832547114 [SQUARE_METRE]
    GrossVolume = 0.00370077030512919 [CUBIC_METRE]
    NetArea = 0.406748832547114 [SQUARE_METRE]
    NetVolume = 0.00370077030512919 [CUBIC_METRE]
  BaseQuantities: 37 more contents on 96 objects not shown
  DATI DA CONTROLLARE | properties | on 64 objects (64 IFCMECHANICALFASTENER)
    DIAMETER = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    HOLE.DIAMETER = 22. (IFCLENGTHMEASURE) [MILLI METRE]
  DATI DA CONTROLLARE | properties | on 6 objects (6 IFCMECHANICALFASTENER)
    DIAMETER = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    HOLE.DIAMETER = 32. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Bolt | properties | on 16 objects (16 IFCMECHANICALFASTENER)
    Bolt Name = "M20*65" (IFCLABEL)
    Bolt count = 3 (IFCINTEGER)
    Bolt hole diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt length = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt size = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt standard = "EN-14399-3" (IFCLABEL)
    Location = "Cantiere" (IFCLABEL)
    Nut count = 3 (IFCINTEGER)
    Nut name = "DADO-20-EN-14399-3" (IFCLABEL)
    Nut type = "14399-3D" (IFCLABEL)
    Slotted hole x = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Slotted hole y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer count = 3 (IFCINTEGER)
    Washer diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer name = "RONDELLA-20-EN-14399-5" (IFCLABEL)
    Washer type = "14399-5" (IFCLABEL)
  Tekla Bolt | properties | on 16 objects (16 IFCMECHANICALFASTENER)
    Bolt Name = "M20*65" (IFCLABEL)
    Bolt count = 4 (IFCINTEGER)
    Bolt hole diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt length = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt size = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt standard = "EN-14399-3" (IFCLABEL)
    Location = "Cantiere" (IFCLABEL)
    Nut count = 4 (IFCINTEGER)
    Nut name = "DADO-20-EN-14399-3" (IFCLABEL)
    Nut type = "14399-3D" (IFCLABEL)
    Slotted hole x = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Slotted hole y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer count = 4 (IFCINTEGER)
    Washer diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer name = "RONDELLA-20-EN-14399-5" (IFCLABEL)
    Washer type = "14399-5" (IFCLABEL)
  Tekla Bolt | properties | on 16 objects (16 IFCMECHANICALFASTENER)
    Bolt Name = "M20*65" (IFCLABEL)
    Bolt count = 6 (IFCINTEGER)
    Bolt hole diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt length = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt size = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt standard = "EN-14399-3" (IFCLABEL)
    Location = "Cantiere" (IFCLABEL)
    Nut count = 6 (IFCINTEGER)
    Nut name = "DADO-20-EN-14399-3" (IFCLABEL)
    Nut type = "14399-3D" (IFCLABEL)
    Slotted hole x = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Slotted hole y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer count = 6 (IFCINTEGER)
    Washer diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer name = "RONDELLA-20-EN-14399-5" (IFCLABEL)
    Washer type = "14399-5" (IFCLABEL)
  Tekla Bolt | properties | on 12 objects (12 IFCMECHANICALFASTENER)
    Bolt Name = "M20*55" (IFCLABEL)
    Bolt count = 4 (IFCINTEGER)
    Bolt hole diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt length = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt size = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt standard = "EN-14399-3" (IFCLABEL)
    Location = "Cantiere" (IFCLABEL)
    Nut count = 4 (IFCINTEGER)
    Nut name = "DADO-20-EN-14399-3" (IFCLABEL)
    Nut type = "14399-3D" (IFCLABEL)
    Slotted hole x = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Slotted hole y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer count = 4 (IFCINTEGER)
    Washer diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer name = "RONDELLA-20-EN-14399-5" (IFCLABEL)
    Washer type = "14399-5" (IFCLABEL)
  Tekla Bolt | properties | on 6 objects (6 IFCMECHANICALFASTENER)
    Bolt Name = "M20*50" (IFCLABEL)
    Bolt count = 4 (IFCINTEGER)
    Bolt hole diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt length = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt size = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt standard = "EN-14399-3" (IFCLABEL)
    Location = "Cantiere" (IFCLABEL)
    Nut count = 0 (IFCINTEGER)
    Nut name = "DADO-20-EN-14399-3" (IFCLABEL)
    Nut type = "14399-3D" (IFCLABEL)
    Slotted hole x = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Slotted hole y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer count = 0 (IFCINTEGER)
    Washer diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer name = "RONDELLA-20-EN-14399-5" (IFCLABEL)
    Washer type = "14399-5" (IFCLABEL)
  Tekla Bolt | properties | on 4 objects (4 IFCMECHANICALFASTENER)
    Bolt Name = "M20*50" (IFCLABEL)
    Bolt count = 4 (IFCINTEGER)
    Bolt hole diameter = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt length = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt size = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Bolt standard = "EN-14399-3" (IFCLABEL)
    Location = "Cantiere" (IFCLABEL)
    Nut count = 4 (IFCINTEGER)
    Nut name = "DADO-20-EN-14399-3" (IFCLABEL)
    Nut type = "14399-3D" (IFCLABEL)
    Slotted hole x = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Slotted hole y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer count = 4 (IFCINTEGER)
    Washer diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Washer name = "RONDELLA-20-EN-14399-5" (IFCLABEL)
    Washer type = "14399-5" (IFCLABEL)
  Tekla Common | properties | on 36 objects (36 IFCDISCRETEACCESSORY)
    Bottom elevation = "+0.010" (IFCLABEL)
    Class = "99" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.210" (IFCLABEL)
  Tekla Common | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    Bottom elevation = "+6.593" (IFCLABEL)
    Class = "99" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+6.613" (IFCLABEL)
  Tekla Common | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    Bottom elevation = "+2.993" (IFCLABEL)
    Class = "99" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+3.013" (IFCLABEL)
  Tekla Common | properties | on 12 objects (12 IFCDISCRETEACCESSORY)
    Bottom elevation = "+4.872" (IFCLABEL)
    Class = "99" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+5.332" (IFCLABEL)
  Tekla Common | properties | on 12 objects (12 IFCDISCRETEACCESSORY)
    Bottom elevation = "+6.880" (IFCLABEL)
    Class = "99" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+7.230" (IFCLABEL)
  Tekla Common | properties | on 12 objects (12 IFCDISCRETEACCESSORY)
    Bottom elevation = "+3.280" (IFCLABEL)
    Class = "99" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+3.630" (IFCLABEL)
  Tekla Common | properties | on 8 objects (8 IFCDISCRETEACCESSORY)
    Bottom elevation = "+6.593" (IFCLABEL)
    Class = "99" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+7.210" (IFCLABEL)
  Tekla Common | properties | on 8 objects (8 IFCDISCRETEACCESSORY)
    Bottom elevation = "+6.606" (IFCLABEL)
    Class = "99" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+6.910" (IFCLABEL)
  Tekla Common: 15 more contents on 84 objects not shown
  Tekla Quantity | properties | on 36 objects (36 IFCDISCRETEACCESSORY)
    Area per tons = 29.4 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 1.4 (IFCMASSMEASURE) [KILO GRAM]
    Width = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 32 objects (32 IFCDISCRETEACCESSORY)
    Area per tons = 15.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 352. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.1 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 7.6 (IFCMASSMEASURE) [KILO GRAM]
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 24 objects (24 IFCDISCRETEACCESSORY)
    Area per tons = 19.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.1 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 244.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 352. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 8.6 (IFCMASSMEASURE) [KILO GRAM]
    Width = 14. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 24 objects (24 IFCDISCRETEACCESSORY)
    Area per tons = 20.1 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 220. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 8.6 (IFCMASSMEASURE) [KILO GRAM]
    Width = 14. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    Area per tons = 14. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 616.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.4 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 29.1 (IFCMASSMEASURE) [KILO GRAM]
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    Area per tons = 19.4 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 276. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 807.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.6 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 71.3 (IFCMASSMEASURE) [KILO GRAM]
    Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 12 objects (12 IFCDISCRETEACCESSORY)
    Area per tons = 20.1 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 244.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 262. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.1 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 6.8 (IFCMASSMEASURE) [KILO GRAM]
    Width = 14. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 8 objects (8 IFCDISCRETEACCESSORY)
    Area per tons = 29.7 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 460. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.1 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 2.5 (IFCMASSMEASURE) [KILO GRAM]
    Width = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity: 8 more contents on 36 objects not shown
  Pset_PlateCommon | properties | on 36 objects (36 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1002" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 32 objects (32 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1005" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1004" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1003" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 12 objects (12 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1010" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 12 objects (12 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1009" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 12 objects (12 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1008" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 12 objects (12 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1007" (IFCIDENTIFIER)
  Pset_PlateCommon: 5 more contents on 34 objects not shown
  Tekla Weld Common | properties | on 64 objects (64 IFCFASTENER)
    Assembly type = "Officina" (IFCLABEL)
    Edge/Around = "Bordo" (IFCLABEL)
    Electrode classification = "No" (IFCLABEL)
    Electrode coefficent = 0. (IFCREAL)
    Electrode strength = 0. (IFCREAL)
    Intermittent type = "Continuo" (IFCLABEL)
    Length = 113. (IFCLENGTHMEASURE) [MILLI METRE]
    NDT inspection level = "No" (IFCLABEL)
    Process type = "No" (IFCLABEL)
    Reference text = "" (IFCLABEL)
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weld comment (no value)
    Weld number = "0" (IFCLABEL)
  Tekla Weld Common | properties | on 48 objects (48 IFCFASTENER)
    Assembly type = "Officina" (IFCLABEL)
    Edge/Around = "Attorno" (IFCLABEL)
    Electrode classification = "No" (IFCLABEL)
    Electrode coefficent = 0. (IFCREAL)
    Electrode strength = 0. (IFCREAL)
    Intermittent type = "Continuo" (IFCLABEL)
    Length = 114.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NDT inspection level = "No" (IFCLABEL)
    Process type = "No" (IFCLABEL)
    Reference text = "" (IFCLABEL)
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weld comment (no value)
    Weld number = "0" (IFCLABEL)
  Tekla Weld Common | properties | on 44 objects (44 IFCFASTENER)
    Assembly type = "Officina" (IFCLABEL)
    Edge/Around = "Bordo" (IFCLABEL)
    Electrode classification = "No" (IFCLABEL)
    Electrode coefficent = 0. (IFCREAL)
    Electrode strength = 0. (IFCREAL)
    Intermittent type = "Continuo" (IFCLABEL)
    Length = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    NDT inspection level = "No" (IFCLABEL)
    Process type = "No" (IFCLABEL)
    Reference text = "" (IFCLABEL)
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weld comment (no value)
    Weld number = "0" (IFCLABEL)
  Tekla Weld Common | properties | on 36 objects (36 IFCFASTENER)
    Assembly type = "Officina" (IFCLABEL)
    Edge/Around = "Attorno" (IFCLABEL)
    Electrode classification = "No" (IFCLABEL)
    Electrode coefficent = 0. (IFCREAL)
    Electrode strength = 0. (IFCREAL)
    Intermittent type = "Continuo" (IFCLABEL)
    Length = 1443. (IFCLENGTHMEASURE) [MILLI METRE]
    NDT inspection level = "No" (IFCLABEL)
    Process type = "No" (IFCLABEL)
    Reference text = "" (IFCLABEL)
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weld comment (no value)
    Weld number = "0" (IFCLABEL)
  Tekla Weld Common | properties | on 36 objects (36 IFCFASTENER)
    Assembly type = "Officina" (IFCLABEL)
    Edge/Around = "Bordo" (IFCLABEL)
    Electrode classification = "No" (IFCLABEL)
    Electrode coefficent = 0. (IFCREAL)
    Electrode strength = 0. (IFCREAL)
    Intermittent type = "Continuo" (IFCLABEL)
    Length = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    NDT inspection level = "No" (IFCLABEL)
    Process type = "No" (IFCLABEL)
    Reference text = "" (IFCLABEL)
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weld comment (no value)
    Weld number = "0" (IFCLABEL)
  Tekla Weld Common | properties | on 36 objects (36 IFCFASTENER)
    Assembly type = "Officina" (IFCLABEL)
    Edge/Around = "Bordo" (IFCLABEL)
    Electrode classification = "No" (IFCLABEL)
    Electrode coefficent = 0. (IFCREAL)
    Electrode strength = 0. (IFCREAL)
    Intermittent type = "Continuo" (IFCLABEL)
    Length = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    NDT inspection level = "No" (IFCLABEL)
    Process type = "No" (IFCLABEL)
    Reference text = "" (IFCLABEL)
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weld comment (no value)
    Weld number = "0" (IFCLABEL)
  Tekla Weld Common | properties | on 32 objects (32 IFCFASTENER)
    Assembly type = "Officina" (IFCLABEL)
    Edge/Around = "Bordo" (IFCLABEL)
    Electrode classification = "No" (IFCLABEL)
    Electrode coefficent = 0. (IFCREAL)
    Electrode strength = 0. (IFCREAL)
    Intermittent type = "Continuo" (IFCLABEL)
    Length = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    NDT inspection level = "No" (IFCLABEL)
    Process type = "No" (IFCLABEL)
    Reference text = "" (IFCLABEL)
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weld comment (no value)
    Weld number = "0" (IFCLABEL)
  Tekla Weld Common | properties | on 32 objects (32 IFCFASTENER)
    Assembly type = "Officina" (IFCLABEL)
    Edge/Around = "Bordo" (IFCLABEL)
    Electrode classification = "No" (IFCLABEL)
    Electrode coefficent = 0. (IFCREAL)
    Electrode strength = 0. (IFCREAL)
    Intermittent type = "Continuo" (IFCLABEL)
    Length = 298. (IFCLENGTHMEASURE) [MILLI METRE]
    NDT inspection level = "No" (IFCLABEL)
    Process type = "No" (IFCLABEL)
    Reference text = "" (IFCLABEL)
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weld comment (no value)
    Weld number = "0" (IFCLABEL)
  Tekla Weld Common: 7 more contents on 134 objects not shown
  Tekla Weld Above Line | properties | on 64 objects (64 IFCFASTENER)
    Actual length1 = 113. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area1 = 4.E-05 (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type1 = "Nessun" (IFCLABEL)
    Finish1 = "Nessun" (IFCLABEL)
    Increment count1 = 0 (IFCINTEGER)
    Length1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch1 = 0. (IFCREAL)
    Root face thickness1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix1 = "" (IFCLABEL)
    Size1 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type1 = "W10" (IFCLABEL)
    Weld angle1 = 0. (IFCREAL)
  Tekla Weld Above Line | properties | on 48 objects (48 IFCFASTENER)
    Actual length1 = 114.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area1 = 4.E-05 (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type1 = "Nessun" (IFCLABEL)
    Finish1 = "Nessun" (IFCLABEL)
    Increment count1 = 0 (IFCINTEGER)
    Length1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch1 = 0. (IFCREAL)
    Root face thickness1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix1 = "" (IFCLABEL)
    Size1 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type1 = "W10" (IFCLABEL)
    Weld angle1 = 0. (IFCREAL)
  Tekla Weld Above Line | properties | on 36 objects (36 IFCFASTENER)
    Actual length1 = 1443. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area1 = 4.E-05 (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type1 = "Nessun" (IFCLABEL)
    Finish1 = "Nessun" (IFCLABEL)
    Increment count1 = 0 (IFCINTEGER)
    Length1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch1 = 0. (IFCREAL)
    Root face thickness1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix1 = "" (IFCLABEL)
    Size1 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type1 = "W10" (IFCLABEL)
    Weld angle1 = 0. (IFCREAL)
  Tekla Weld Above Line | properties | on 36 objects (36 IFCFASTENER)
    Actual length1 = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area1 = 4.E-05 (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type1 = "Nessun" (IFCLABEL)
    Finish1 = "Nessun" (IFCLABEL)
    Increment count1 = 0 (IFCINTEGER)
    Length1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch1 = 0. (IFCREAL)
    Root face thickness1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix1 = "" (IFCLABEL)
    Size1 = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Type1 = "W10" (IFCLABEL)
    Weld angle1 = 0. (IFCREAL)
  Tekla Weld Above Line | properties | on 36 objects (36 IFCFASTENER)
    Actual length1 = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area1 = 4.E-05 (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type1 = "Nessun" (IFCLABEL)
    Finish1 = "Nessun" (IFCLABEL)
    Increment count1 = 0 (IFCINTEGER)
    Length1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch1 = 0. (IFCREAL)
    Root face thickness1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix1 = "" (IFCLABEL)
    Size1 = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Type1 = "W10" (IFCLABEL)
    Weld angle1 = 0. (IFCREAL)
  Tekla Weld Above Line | properties | on 32 objects (32 IFCFASTENER)
    Actual length1 = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area1 = 4.E-05 (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type1 = "Nessun" (IFCLABEL)
    Finish1 = "Nessun" (IFCLABEL)
    Increment count1 = 0 (IFCINTEGER)
    Length1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch1 = 0. (IFCREAL)
    Root face thickness1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix1 = "" (IFCLABEL)
    Size1 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type1 = "W10" (IFCLABEL)
    Weld angle1 = 0. (IFCREAL)
  Tekla Weld Above Line | properties | on 32 objects (32 IFCFASTENER)
    Actual length1 = 298. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area1 = 4.E-05 (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type1 = "Nessun" (IFCLABEL)
    Finish1 = "Nessun" (IFCLABEL)
    Increment count1 = 0 (IFCINTEGER)
    Length1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch1 = 0. (IFCREAL)
    Root face thickness1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix1 = "" (IFCLABEL)
    Size1 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type1 = "W10" (IFCLABEL)
    Weld angle1 = 0. (IFCREAL)
  Tekla Weld Above Line | properties | on 32 objects (32 IFCFASTENER)
    Actual length1 = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area1 = 4.E-05 (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type1 = "Nessun" (IFCLABEL)
    Finish1 = "Nessun" (IFCLABEL)
    Increment count1 = 0 (IFCINTEGER)
    Length1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch1 = 0. (IFCREAL)
    Root face thickness1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix1 = "" (IFCLABEL)
    Size1 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type1 = "W10" (IFCLABEL)
    Weld angle1 = 0. (IFCREAL)
  Tekla Weld Above Line: 8 more contents on 146 objects not shown
  Tekla Weld Below Line | properties | on 180 objects (180 IFCFASTENER)
    Actual length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area2 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type2 = "Nessun" (IFCLABEL)
    Finish2 = "Nessun" (IFCLABEL)
    Increment count2 = 0 (IFCINTEGER)
    Length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch2 = 0. (IFCREAL)
    Root face thicness2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix2 = "" (IFCLABEL)
    Size2 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type2 = "Nessun" (IFCLABEL)
    Weld angle2 = 0. (IFCREAL)
  Tekla Weld Below Line | properties | on 64 objects (64 IFCFASTENER)
    Actual length2 = 113. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area2 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type2 = "Nessun" (IFCLABEL)
    Finish2 = "Nessun" (IFCLABEL)
    Increment count2 = 0 (IFCINTEGER)
    Length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch2 = 0. (IFCREAL)
    Root face thicness2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix2 = "" (IFCLABEL)
    Size2 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type2 = "W10" (IFCLABEL)
    Weld angle2 = 0. (IFCREAL)
  Tekla Weld Below Line | properties | on 36 objects (36 IFCFASTENER)
    Actual length2 = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area2 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type2 = "Nessun" (IFCLABEL)
    Finish2 = "Nessun" (IFCLABEL)
    Increment count2 = 0 (IFCINTEGER)
    Length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch2 = 0. (IFCREAL)
    Root face thicness2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix2 = "" (IFCLABEL)
    Size2 = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Type2 = "W10" (IFCLABEL)
    Weld angle2 = 0. (IFCREAL)
  Tekla Weld Below Line | properties | on 36 objects (36 IFCFASTENER)
    Actual length2 = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area2 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type2 = "Nessun" (IFCLABEL)
    Finish2 = "Nessun" (IFCLABEL)
    Increment count2 = 0 (IFCINTEGER)
    Length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch2 = 0. (IFCREAL)
    Root face thicness2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix2 = "" (IFCLABEL)
    Size2 = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Type2 = "W10" (IFCLABEL)
    Weld angle2 = 0. (IFCREAL)
  Tekla Weld Below Line | properties | on 32 objects (32 IFCFASTENER)
    Actual length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area2 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type2 = "Nessun" (IFCLABEL)
    Finish2 = "Nessun" (IFCLABEL)
    Increment count2 = 0 (IFCINTEGER)
    Length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch2 = 0. (IFCREAL)
    Root face thicness2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix2 = "" (IFCLABEL)
    Size2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type2 = "Nessun" (IFCLABEL)
    Weld angle2 = 0. (IFCREAL)
  Tekla Weld Below Line | properties | on 32 objects (32 IFCFASTENER)
    Actual length2 = 298. (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area2 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type2 = "Nessun" (IFCLABEL)
    Finish2 = "Nessun" (IFCLABEL)
    Increment count2 = 0 (IFCINTEGER)
    Length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch2 = 0. (IFCREAL)
    Root face thicness2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix2 = "" (IFCLABEL)
    Size2 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type2 = "W10" (IFCLABEL)
    Weld angle2 = 0. (IFCREAL)
  Tekla Weld Below Line | properties | on 32 objects (32 IFCFASTENER)
    Actual length2 = 291.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area2 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type2 = "Nessun" (IFCLABEL)
    Finish2 = "Nessun" (IFCLABEL)
    Increment count2 = 0 (IFCINTEGER)
    Length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch2 = 0. (IFCREAL)
    Root face thicness2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix2 = "" (IFCLABEL)
    Size2 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type2 = "W10" (IFCLABEL)
    Weld angle2 = 0. (IFCREAL)
  Tekla Weld Below Line | properties | on 16 objects (16 IFCFASTENER)
    Actual length2 = 291.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Cross section area2 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Effective throat2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Fill type2 = "Nessun" (IFCLABEL)
    Finish2 = "Nessun" (IFCLABEL)
    Increment count2 = 0 (IFCINTEGER)
    Length2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Pitch2 = 0. (IFCREAL)
    Root face thicness2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Root opening2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Size prefix2 = "" (IFCLABEL)
    Size2 = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Type2 = "W10" (IFCLABEL)
    Weld angle2 = 0. (IFCREAL)
  Tekla Weld Below Line: 3 more contents on 34 objects not shown
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P/6" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P/3" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P/2" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P/1" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P/5" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "P/4" (IFCIDENTIFIER)