IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "RevitIdentifiers [VersionGUID: 9c111974-55d2-4a0d-b08f-9e566549ab4c, NumberOfSaves: 1]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates, ProjectSite: Default Site]"
Description: "ExchangeRequirement [Architecture]"
Time stamp: "2023-07-10T10:24:44+01:00"
Preprocessor: "ODA SDAI 23.12"
Originating system: "Autodesk Revit 24.0.20.20 (ENG) - IFC 24.1.0.22"
Application: "Autodesk Revit 2024 (ENG)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENG)"

People and organizations
  Person "dirk.vanrillaer@rijksoverheid.nl" of Organization (no name given)
  Owner history of Person "dirk.vanrillaer@rijksoverheid.nl" of Organization (no name given) | application "Autodesk Revit 2024 (ENG)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENG)" | change NOCHANGE | created 1688977213 (2023-07-10T08:20:13Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  AREADENSITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 5 elements
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:Wall 1" | object type "Basic Wall:Wall 1" | names: "Basic Wall:Wall 1:2984", "Basic Wall:Wall 1:3046", "Basic Wall:Wall 1:3164" (+1 more) | material: "Default Wall" | property sets: Qto_WallBaseQuantities, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:Wall 2" | object type "Basic Wall:Wall 2" | names: "Basic Wall:Wall 2:3745" | material: "Default Wall" | property sets: Qto_WallBaseQuantities, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Types
  IFCWALLTYPE "Basic Wall:Wall 1" | STANDARD | 4 occurrences | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:Wall 2" | STANDARD | 1 occurrence | property sets: Pset_WallCommon

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.0400000000000007 [SQUARE_METRE]
    GrossSideArea = 20.800000000000008 [SQUARE_METRE]
    GrossVolume = 4.1600000000000019 [CUBIC_METRE]
    Height = 3999.9999999999995 [MILLI METRE]
    Length = 5200.0000000000036 [MILLI METRE]
    NetSideArea = 20.800000000000008 [SQUARE_METRE]
    NetVolume = 4.1600000000000028 [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.50000000000000011 [SQUARE_METRE]
    GrossSideArea = 10.000000000000002 [SQUARE_METRE]
    GrossVolume = 2.0000000000000004 [CUBIC_METRE]
    Height = 4000.0000000000005 [MILLI METRE]
    Length = 2500. [MILLI METRE]
    NetSideArea = 10.000000000000002 [SQUARE_METRE]
    NetVolume = 2. [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.99999999999999889 [SQUARE_METRE]
    GrossSideArea = 19.999999999999975 [SQUARE_METRE]
    GrossVolume = 3.999999999999996 [CUBIC_METRE]
    Height = 4000.0000000000005 [MILLI METRE]
    Length = 4999.9999999999936 [MILLI METRE]
    NetSideArea = 19.999999999999975 [SQUARE_METRE]
    NetVolume = 3.9999999999999929 [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.46000000000000019 [SQUARE_METRE]
    GrossSideArea = 9.2000000000000011 [SQUARE_METRE]
    GrossVolume = 1.8400000000000005 [CUBIC_METRE]
    Height = 3999.9999999999995 [MILLI METRE]
    Length = 2300.0000000000009 [MILLI METRE]
    NetSideArea = 9.2000000000000011 [SQUARE_METRE]
    NetVolume = 1.8400000000000005 [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.23000000000000009 [SQUARE_METRE]
    GrossSideArea = 9.2000000000000011 [SQUARE_METRE]
    GrossVolume = 0.92000000000000026 [CUBIC_METRE]
    Height = 3999.9999999999995 [MILLI METRE]
    Length = 2300.0000000000009 [MILLI METRE]
    NetSideArea = 9.2000000000000011 [SQUARE_METRE]
    NetVolume = 0.92000000000000004 [CUBIC_METRE]
    Width = 100. [MILLI METRE]
  Pset_EnvironmentalImpactIndicators | properties | on 4 objects (4 IFCWALL)
    Reference = "Wall 1" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCWALL)
    Reference = "Wall 2" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALL)
    Reference = "Wall 1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Wall 2" (IFCLABEL)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall 1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall 2" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDINGSYSTEM)
    Reference = "buitenschil" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Level 1" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)