IFC building model
Schema: "IFC4"
Description: "ViewDefinition [Design_Transfer_View]"
Description: "ExchangeRequirement [Architecture]"
Description: "Option [Drawing Scale: 100.000000]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and ARCHICAD 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: Off]"
Description: "Option [Export geometries that Participates in Collision Detection only: Off]"
Description: "Option [Split complex elements: Off]"
Description: "Option [Material Preservation: Explode where necessary]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [Slabs with slanted edge(s): Extruded]"
File name: "C:\Users\xx\Desktop\indexedpolycurve.ifc"
Time stamp: "2020-09-15T15:07:33"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.09 : 26 Sep 2013"
Originating system: "IFC file generated by GRAPHISOFT ARCHICAD 24.0.0 INT FULL Windows version (IFC add-on version: 3008 INT FULL)."
Authorization: "The authorising person"
Application: "ARCHICAD" version "24.0.0" identifier "IFC add-on version: 3008 INT FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT"

People and organizations
  Person "Undefined" of Organization "Undefined"
  Owner history of Person "Undefined" of Organization "Undefined" | application "ARCHICAD" version "24.0.0" identifier "IFC add-on version: 3008 INT FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT" | change NOCHANGE | created 1600175253 (2020-09-15T13:07:33Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  CURRENCY: USD
  TIMEUNIT: Year (conversion based)
  MASSUNIT: KILO GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  ENERGYUNIT: MEGA JOULE
  THERMALCONDUCTANCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "Project"
  IFCSITE "Site" | latitude 47° 33′ 34.9488″ | longitude 19° 3′ 17.2044″ | elevation above sea level 0.
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "Ground Floor" | elevation 0.
        contains 3 elements
          2 x IFCWALL | type IFCWALLTYPE "Generic Wall/Shell 300" | names: "SW - 001", "SW - 002" | material: layers "Generic Wall/Shell" ("GENERIC - EXTERNAL CLADDING" 50., "GENERIC - STRUCTURAL" 250.) | property sets: Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "GENERIC - STRUCTURAL 300 x 300" | COLUMN | names: "CRE - 001" | material: "GENERIC - STRUCTURAL" | property sets: Pset_ColumnCommon

Types
  IFCWALLTYPE "Generic Wall/Shell 300" | 2 occurrences
  IFCCOLUMNTYPE "GENERIC - STRUCTURAL 300 x 300" | COLUMN | 1 occurrence

Property sets
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    Status in {"NEW"} (IFCLABEL)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    Reference = "GENERIC - STRUCTURAL 300 x 300" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Status in {"NEW"} (IFCLABEL)