IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "out.ifc"
Time stamp: "2021-02-25T09:42:30"
Author: "TAKENAKA\0600731"
Organization: "Structural Designer"
Preprocessor: "IFC Database version:Work"
Originating system: "Tekla Structures 2017 Service Pack 9, IFC Export Version: 4.0.0.0 Sep 19 2018"
Application: "Tekla Structures" version "2017 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

People and organizations
  Person "Undefined" id "TAKENAKA\0600731" of Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "TAKENAKA\0600731" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2017 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1614213750 (2021-02-25T00:42:30Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Tekla Structures"
  IFCSITE "Undefined" | elevation above sea level 0.
    IFCBUILDING "Undefined"
      contains 2 elements
        2 x IFCGRID | names: "R", "1"
      IFCBUILDINGSTOREY "1" | elevation 0.
        contains 1 element
          1 x IFCBEAM | type IFCBEAMTYPE "CON□650*350" | object type "CON□650*350" | names: "1GA1" | descriptions: "CON□650*350" | material: "CONCRETE/FC24" | property sets: Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities

Types
  IFCBEAMTYPE "CON□650*350" | 1 occurrence

Property sets
  Tekla Common | properties | on 1 object (1 IFCBEAM)
    Bottom elevation = "-0.650" (IFCLABEL)
    Class = "8" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.000" (IFCLABEL)
  Tekla Quantity | properties | on 1 object (1 IFCBEAM)
    Area per tons = 3.7 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 2.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 650. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 16.5 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.8 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 4268.5 (IFCMASSMEASURE) [KILO GRAM]
    Width = 350. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "G-0(?)" (IFCIDENTIFIER)
  BaseQuantities | quantities | on 1 object (1 IFCBEAM)
    Length = 8000. [MILLI METRE]
    NetVolume = 1.82 [CUBIC_METRE]
    NetWeight = 4268.537 [KILO GRAM]
    OuterSurfaceArea = 16. [SQUARE_METRE]