IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2021-02-25T09:27:54"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.12.1 - 代替 UI 20.2.12.1"
Application: "Autodesk Revit 2020 (JPN)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (JPN)"

People and organizations
  Person "marukawa.tomoki@takenaka.co.jp" of Organization "RevitUserGroup"
  Owner history of Person "marukawa.tomoki@takenaka.co.jp" of Organization "RevitUserGroup" | application "Autodesk Revit 2020 (JPN)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (JPN)" | change NOCHANGE | created 1614212871 (2021-02-25T00:27:51Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 35° 41′ 22.154846″ | longitude 139° 41′ 30.161132″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "1FL" | long name "1FL" | object type "レベル:レベル 上表示" | elevation 0.
        contains 1 element
          1 x IFCBEAM | type IFCBEAMTYPE "1GA1" | object type "RC_G:1GA1" | names: "RC_G:1GA1:383152" | material: "コンクリート-CONCR Fc24" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam

Types
  IFCBEAMTYPE "1GA1" | BEAM | 1 occurrence | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam

Property sets
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1GA1" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 8000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1GA1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBEAM) | on 1 type object
    Reference = "1GA1" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 object (1 IFCBEAM) | on 1 type object
    Reference = "1GA1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)

Other addresses and roles
  2 x postal address: "住所", "東京、日本"