IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
File name: "1000"
Time stamp: "2022-02-11T10:33:03"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.11.27 - Exporter 21.1.11.27 - Alternate UI 21.1.11.27"
Application: "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)"

People and organizations
  Person "kalleUBA5S" of Organization "Koostaja OÜ" description "Inseneribüroo"
  Owner history of Person "kalleUBA5S" of Organization "Koostaja OÜ" description "Inseneribüroo" | application "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)" | change NOCHANGE | created 1644332773 (2022-02-08T15:06:13Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "1000" | long name "Näidisprojekt" | phase "EP"
  IFCSITE "Default" | latitude 59° 26′ 11.044921″ | longitude 24° 45′ 9.146118″ | elevation above sea level 0.
    IFCBUILDING "Hoone 1" | long name "Hoone 1" | postal address: "Näidise tee 1 00000 Maakond Eesti", "Tallinn", "Estonia"
      IFCBUILDINGSTOREY "1 korrus" | long name "1 korrus" | object type "Level:Name, elevation(Survey)" | elevation 0.
        contains 4 elements
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:VS-01" | object type "Basic Wall:VS-01" | names: "Basic Wall:VS-01:81844" | material: layers "Basic Wall:VS-01" ("EST. Betoon. Armeeritud. C30/37" 0.2) | property sets: EK_Sein
          1 x IFCSLAB | type IFCSLABTYPE "Floor:VL-01" | object type "Floor:VL-01" | FLOOR | names: "Floor:VL-01:81895" | material: layers "Floor:VL-01" ("EST. Betoon. Armeeritud. C30/37" 0.08, "EST. Soojustus. Kivivill. Default" 0.05, "EST. Betoon. Armeeritud. C30/37" 0.265) | property sets: EK_Vahelagi
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "RB nelikant post:450 x 600mm" | object type "RB nelikant post:450 x 600mm" | COLUMN | names: "RB nelikant post:450 x 600mm:88580" | material: "EST. Betoon. Armeeritud. C30/37" | property sets: EK_Tala-Post
          1 x IFCPILE | type IFCPILETYPE "Kohtvai:Kohtvai" | object type "Kohtvai:Kohtvai" | names: "Kohtvai:Kohtvai:93180" | material: "EST. Betoon. Armeeritud. C30/37" | property sets: EK_Vundament

Types
  IFCWALLTYPE "Basic Wall:VS-01" | 1 occurrence | material: layers "Basic Wall:VS-01" ("EST. Betoon. Armeeritud. C30/37" 0.2) | property sets: EK_Sein
  IFCSLABTYPE "Floor:VL-01" | FLOOR | 1 occurrence | material: layers "Floor:VL-01" ("EST. Betoon. Armeeritud. C30/37" 0.08, "EST. Soojustus. Kivivill. Default" 0.05, "EST. Betoon. Armeeritud. C30/37" 0.265) | property sets: EK_Vahelagi
  IFCCOLUMNTYPE "RB nelikant post:450 x 600mm" | COLUMN | 1 occurrence | material: "EST. Betoon. Armeeritud. C30/37" | property sets: EK_Tala-Post
  IFCPILETYPE "Kohtvai:Kohtvai" | 1 occurrence | material: "EST. Betoon. Armeeritud. C30/37" | property sets: EK_Vundament

Property sets
  EK_Sein | properties | on 1 object (1 IFCWALL)
    001_Nimetus = "Välissein" (IFCLABEL)
    002_Tähis = "VS-01" (IFCIDENTIFIER)
    105_Tugevusklass = "C30/37" (IFCLABEL)
    110_Keskkonnaklass = "XC3+XF1" (IFCLABEL)
    111_Armeerimistegur = 0.0035 (IFCREAL)
    120_Materjal = "Monoliitne raudbetoon" (IFCLABEL)
    135_Ruumala = 4.672 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    150_Paksus = 0.2 (IFCLENGTHMEASURE) [METRE]
    155_Bruto_pindala = 24. (IFCAREAMEASURE) [SQUARE_METRE]
    160_Neto_pindala = 23.36 (IFCAREAMEASURE) [SQUARE_METRE]
    190_Ülemine_kõrgusmärk = 4. (IFCLENGTHMEASURE) [METRE]
    195_Alumine_kõrgusmärk = 0. (IFCLENGTHMEASURE) [METRE]
  EK_Sein | properties | on 1 type object
    002_Tähis = "VS-01" (IFCIDENTIFIER)
    150_Paksus = 0.2 (IFCLENGTHMEASURE) [METRE]
  EK_Vahelagi | properties | on 1 object (1 IFCSLAB)
    001_Nimetus = "Vahelagi" (IFCLABEL)
    002_Tähis = "VL-01" (IFCIDENTIFIER)
    105_Tugevusklass = "C35/45" (IFCLABEL)
    110_Keskkonnaklass = "XC1+XF2" (IFCLABEL)
    120_Materjal = "Monoliitne raudbetoon" (IFCLABEL)
    135_Ruumala = 5.58925 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    150_Paksus = 0.395 (IFCLENGTHMEASURE) [METRE]
    155_Bruto_pindala = 14.4 (IFCAREAMEASURE) [SQUARE_METRE]
    160_Neto_pindala = 14.15 (IFCAREAMEASURE) [SQUARE_METRE]
    190_Ülemine_kõrgusmärk = 6. (IFCLENGTHMEASURE) [METRE]
    195_Alumine_kõrgusmärk = 5.605 (IFCLENGTHMEASURE) [METRE]
  EK_Vahelagi | properties | on 1 type object
    002_Tähis = "VL-01" (IFCIDENTIFIER)
  EK_Tala-Post | properties | on 1 object (1 IFCCOLUMN)
    001_Nimetus = "Raudbetoonpost" (IFCLABEL)
    003_Ristlõige = "450x600" (IFCIDENTIFIER)
    105_Tugevusklass = "C30/37" (IFCLABEL)
    110_Keskkonnaklass = "XC2" (IFCLABEL)
    111_Armeerimistegur = 0.0035 (IFCREAL)
    120_Materjal = "Monteeritav raudbetoon" (IFCLABEL)
    125_Positsioon = "AA/77" (IFCLABEL)
    130_Pikkus = 4.5 (IFCLENGTHMEASURE) [METRE]
    135_Ruumala = 1.215 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    140_Mass = 3037.5 (IFCMASSMEASURE) [KILO GRAM]
    146_Täispindala = 9.45 (IFCAREAMEASURE) [SQUARE_METRE]
    190_Ülemine_kõrgusmärk = 4.5 (IFCLENGTHMEASURE) [METRE]
    195_Alumine_kõrgusmärk = 0. (IFCLENGTHMEASURE) [METRE]
  EK_Tala-Post | properties | on 1 type object
    003_Ristlõige = "450x600" (IFCIDENTIFIER)
  EK_Vundament | properties | on 1 object (1 IFCPILE)
    001_Nimetus = "Kohtvai" (IFCLABEL)
    003_Ristlõige = "D=600" (IFCIDENTIFIER)
    105_Tugevusklass = "C30/37" (IFCLABEL)
    110_Keskkonnaklass = "XF4" (IFCLABEL)
    120_Materjal = "Monoliitne raudbetoon" (IFCLABEL)
    125_Positsioon = "AA/11" (IFCLABEL)
    135_Ruumala = 2.59229188042796 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    145_Pindala = 0.283 (IFCAREAMEASURE) [SQUARE_METRE]
    190_Ülemine_kõrgusmärk = 0.9 (IFCLENGTHMEASURE) [METRE]
    195_Alumine_kõrgusmärk = -6. (IFCLENGTHMEASURE) [METRE]
  EK_Vundament | properties | on 1 type object
    003_Ristlõige = "D=600" (IFCIDENTIFIER)